"GLL"
"Format", "3D"
"FormatVersion", "1.02"

"System", "ULTRA-X82 40H x 50V", "ULTRAX82 40H50V", "LS"
"SystemVersion", 1.00
"Company", "Meyer Sound Laboratories, Inc."

"InfoText", "The ULTRA-X80 and ULTRA-X82 are the most capable models of the Ultra Series point source loudspeakers. These models have been designed for a variety of high-power applications. From sports arenas and stadiums to houses of worship, theaters, and live music venues, the ULTRA-X80 delivers exceptional sonic experiences for all kinds of audiences, in all kinds of venues, for all kinds of sound.\r\n\r\nFeatures:\r\n- Constant directivity rotatable horn\r\n- Concentric driver configuration\r\n- Rigging points top and bottom for mounting and accessory attachment\r\n- Available in custom colors\r\n- Standard and Outdoor Temporary weather protection versions\r\n\r\nThe ULTRA-X80 and ULTRA-X82 have different horn dispersions, 95 x 40 degrees and 50 x 40 degrees, respectively. The horns are rotatable, allowing the cabinet to be mounted horizontally or vertically while maintaining the desired coverage.\r\n\r\nThe durable trapezoidal enclosure of the ULTRA-X80 ships with a slightly textured black finish and is also available in custom colors. A powder-coated, perforated steel grille provides protection to the front of the loudspeakers. Two versions of environmental protection are available for ULTRA-X80: Standard and Outdoor Temporary. The Outdoor Temporary versions of ULTRA-X80 loudspeakers include additional treatment of the wood cabinet and the addition of stainless-steel mesh behind the grille.\r\n\r\nThe ULTRA-X80 is designed to be deployed alongside Meyer Sound LFC series products, extending the low-frequency performance.\r\n\r\nThe high-output switch-mode power supply reduces weight and is more efficient than linear power supplies. The operating voltage is 200-240 V AC, 50-60 Hz. When an appropriately sized and specified branch circuit breaker is in line, multiple ULTRA-X80 loudspeakers can be connected to one circuit.\r\n\r\nBoth analog and Milan AVB audio inputs are provided on the user panel. The connectors provided are from Neutrik’s TRUE1 TOP (True Outdoor Protection) product line. An IP65 rating is achieved for the connectors only when the connected cables are also terminated with Neutrik TRUE1 TOP connectors or when the sealing caps are properly seated when not in use. Each loudspeaker ships with Neutrik TRUE1 TOP cable-mount connectors that mate with the user panel connectors (AC inlet, analog audio, and network)."
"CopyrightText", "© 2025 Meyer Sound Laboratories, Inc. All Rights Reserved."
"SupportText", "See ULTRA-X80 Operating Instructions for support.\r\nhttps://docs.meyersound.com/products/en/operating-instructions---ultra-x80.html"
"WebsiteText", "www.meyersound.com/products"
"EmailText", "info@meyersound.com"


"Logo1", "C:\Users\Public\Documents\EASE40Data\GLL Projects\Meyer Sound\EASE_product_names_new\ms_logo.png"
"Logo2", "C:\Users\Public\Documents\EASE40Data\GLL Projects\Meyer Sound\EASE_product_names_new\241205_ease_ultra-x82_40x50.png"
"BackgroundColor", -1

"BoxTypes", 1
    "BoxType", "ULTRA-X80", "ULTRA-X80"
        "Horizontal Opening Angle", 110
        "Vertical Opening Angle", 50
        "Sources", 1
            "Source", "Source", "Source", 0.00, 0.00, -0.48, 0.00, 0.00, 0.00, "ULTRA-X82_40h50v"
        "Input Configurations", 1
            "Input Configuration", "Default", "InputConfigA"
                "Inputs", 1
                    "Input", "Input"
                        "Rated Impedance", 8.00
                        "Links", 1
                            "Link", "Source", ""
        "GeometryFiles", 1
            "GeometryFile", "C:\Users\Public\Documents\EASE40Data\GLL Projects\Meyer Sound\ULTRAX80_40H95V\Drawings\X80 3D EASE.fed"
        "ReferencePoint", 0.00, 0.00, -0.48
        "NextPivot", 0.00, 0.00, -0.90
        "CenterOfMass", 0.00, 0.32, -0.43
        "Weight", 62.60


"SourceDefinitions", 1
    "SourceDefinition", "ULTRA-X82_40h50v"
        "File", ".\Sources\ULTRA-X82_40h50v.gss"


"FilterGroups", 0

"Presets", 0

"Additional Data Files", 1
    "Additional Data File", "Product Datasheet", "Product Datasheet"
        "File", "C:\Users\Public\Documents\EASE40Data\GLL Projects\Meyer Sound\ULTRAX80_40H95V\datasheet-ultra-x-80.pdf"


"Authorization Files", 1
    "Authorization File", "C:\Users\Public\Documents\EASE40Data\GLL Projects\Meyer Sound\Meyer Sound Laboratories, Inc..author"


